Recording paused.






USAGE...........................................................
Used in the system wide record facility to inform the caller 
they have entered pause mode during the record operation.
